**Titus Displacement Ventilation,**

**DVR1**

**Specification texts**

DVR1 diffuser for low flow air-conditioning is suitable for vertical installation in steps. The unit consists of a rectangular perforated front cover of powder coated galvanealed sheet metal, 18 gauge.  Front cover painted to Titus White #26. DVR1 is available for quick-installation with mounting clips for flush amount or fastened to the surface for exposed mount. Adjustable pattern controllers with radial air deflection blades create a highly inductive adjacent zone for quick reduction of air velocity. Pattern controllers are made of 22 gauge sheet metal painted black Titus #01.  Housing frame suited to fit the nominal width and height in a staircase opening, and made of 18 gauge sheet metal.  DVR1 offered in standard sizes and special sizes.

Panel design, with screw mounting,   max dimensions          \_84\_\_ / \_\_40\_\_ x \_\_N/A\_

With concealed mounting, max dimensions    \_84\_\_ / \_\_40\_\_ x \_\_N/A\_