ECM Specifiable text

* **ECM 3 Speed Offering**

Provide Electronically Commutated (EC) Motor capable of operation with 3 speed thermostat.

**OR**

* **ECM offering**

Provide Electronically Commutated (EC) Motor capable of operation with 3 speed thermostat. Each speed shall be manually adjustable in the field. All manual speed adjustments shall be stored in non-volatile memory.

**OR**

* **ECM offering**

Provide Electronically Commutated (EC) Motor capable of variable speed operation. Motor shall be capable of accepting a 2-10 VDC output from BAS